To whom it may concern

The sealing mechanism for Jomar TG series globe style balancing valves are as follows:

|  |  |  |
| --- | --- | --- |
| **PN** | **Size** | **Type of Seats** |
| TG-BFF | 3/4" | Metal to Metal |
| TG-CFF | 1" | PTFE |
| TG-DFF | 1-1/4" | PTFE |
| TG-EFF | 1-1/2" | PTFE |
| TG-FFF | 2" | EPDM Coated Disk |
| TG-IFF | 4" | EPDM Coated Disk |
| TGV-KFF | 6" | EPDM Gasket |

If there are any additional questions feel free to contact me.

**Nick Miller**  
Engineering Manager

**P** 586.268.1220

**C** 989.878.2105

[](http://www.jomar.com/)